	
	
	WEST MIDLANDS INFLATABLES
PUNCH BAG MACHINE – RISK ASSESSMENT
	
	

	Hazard 
	︎︎︎ Who is at risk? 
	Possible effects/ harm 
	Likelihood (high, medium, low) 
	Evaluation & Control Measures 
	Revised risk rating (high, medium, low) 
	Are there adequate control measures in place? 

	Loading, handling and transportati on of equipment 
	Operator, spectator 
	Injury 
	Low 
	All staff to be trained in manual handling. Manual handling to be reduced to a minimum by use of trollies/lifts. Loads to be properly secured. Where required, multiple persons must handle equipment. 
	Low 
	Yes 

	Installation of equipment on site 
	Operator, spectator, participants 
	Injury to operator, spectators or participants. Damage to venue. 
	Low 
	Operator must have clear, unhindered access to the setup area. Setup area to be clear and free from debris. 
Pre setup checks on equipment to check for damage. Equipment to be set up away from sources of water. 
	Low 
	Yes 



	Ground type 
	Operator, spectator, participants 
	Injury to operator, spectators or participants. 
	Low 
	Equipment to be installed and operated on a hard, level surface. 
	Low 
	Yes 

	Electricity and cabling 
	Operator, spectator, participants 
	Injury to operator, spectators or participants. 
	Medium 
	Item requires access to 13 amp plug socket. Power source should be no more that 25m away from equipment. All cabling to be covered where required and routed away from walkways etc. 
All electrical components to be regularly checked and covered by a PAT test. 
	Low 
	Yes 

	Operation of equipment on site 
	Spectator, participants 
	Injury to spectators or participants. 
	Low 
	Spectators not allowed in the operational area whilst someone is participating. Spectators to be kept at a distance from the equipment and not allowed to sit/rest, or interfere with the equipment in any way. 
	Low 
	Yes 



	Hazard
	Who is at Risk?
	Possible/effects/harm
	Likelihood (high, medium, low)
	Evaluation & Control Measures 
	Revised risk rating    (high, medium, low) 
	Are there adequate control measures in plave?

	User safety 
	Organiser, spectator, participants 
	Injury to organiser, spectators or participants. 
	Low 
	[bookmark: _GoBack]Any participants under the influence of alcohol/ drugs to the extent where they are posing a risk to spectators or themselves should not be allowed to participate. Children to be supervised by an adult at all times. Maximum of 1 user per game is permitted. Participants should be aware of their own physical ability and should not use the equipment if suffering from any pre- existing injuries/ conditions. 
	Low 
	Yes 

	Heat 
	Organiser, spectator, participants 
	Injury to spectators or participants. 
	Low 
	The equipment should not be set up near any sources of heat or naked flames. 
	Low 
	Yes 

	Weather
	Organiser, spectator,participants
	Slip/Trip
	Low
	The equipment can only be used indoors, in a dry environment, away from any sources of water/ humidity/ cold
	Low
	Yes



Risk rating High 
For example: 
fatality possible to one or more individuals however infrequent major injury to few individuals occurring frequently 
likelihood of long term muscular-skeletal problems affecting significant numbers of staff
Immediate action required 
Medium 
For example: 
major injury to one/few individuals occurring infrequently 
likelihood of long term muscular-skeletal problems affecting some staff. Requires attention as soon as possible 
• Low 
For example: 
• minor injury occurring infrequently to few staff.
Not a priority, may need attention if not as low as reasonably practicable. 
major injury to one/few individuals occurring infrequently 
likelihood of long term muscular-skeletal problems affecting some staff. Requires attention as soon as possible 


